Specification

Model No.: 		PHL4108
Input: 			220-240V, 50-60Hz
Sensor Type:		PIR
Max:			2000W incandescent, 
			600W fluorescent
			200W LED lamp
Rating: 		IP20
Cut-out:		Ø63mm
Fitting Colour:		White, Black and Brush Chrome 
Detection Area:		about 360°, radius 4.5m (when installed 2.8m high) 
Duration Time: 		10+/-5 seconds to 4+/-1 minutes adjustable
Lux Control:		Daylight and night adjustable
Sensitive Adjustable:	No
Override Function:	No
       			 
       			 
       			


